Name\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Donning and Doffing SCBA Quiz**

1. Which of the following is the most common method of donning SCBA?
   1. Over-the-head method
   2. Coat method
   3. Seat-mounted method
   4. All of the above
2. According to NFPA 1404, a full SCBA cylinder is filled to no less than \_\_\_\_\_% of its rated capacity.
3. 70
4. 75
5. 80
6. 90
7. When checking an SCBA unit, check the remote gauge and cylinder gauge to ensure they read within \_\_\_\_\_\_\_\_ psi.
8. 100
9. 200
10. 300
11. 500
12. When donning the SCBA using the over-the-head method, position the SCBA with the cylinder valve end \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_.
13. Towards you
14. Next to you
15. Away from you
16. At your side
17. When donning the SCBA, always open the cylinder valve fully.
18. True
19. False
20. An advantage of seat-mounted SCBA is that you can don it en route to an incident.
21. True
22. False
23. It is safe and proper to interchange SCBA components from different manufacturers.
24. True
25. False
26. Firefighters should not wear a beard because \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_.
27. It looks shabby
28. It interferes with the SCBA facepiece seal
29. Firefighters may wear beards
30. None of the above
31. Which of the following is NOT an action that applies to doffing all SCBA?
32. Activate your PASS device
33. Make sure you are out of the contaminated area
34. Close the cylinder valve
35. Discontinue air flow from the regulator to the facepiece
36. When changing cylinders, which of the following should be placed on the ground to protect the spare cylinders?
37. Carrying case
38. Section of hose
39. Salvage cover
40. None of the above