**Filling the Gap Quiz Key**

Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. **True** or False Care should be taken not to burn through the wall of the tubing.

2. **True** or False Weld an overlapping bead across the original pass.

3. True or **False** Complete this process until there is just a small hole in the gap.

4. True or **False** You should grind off the weld with an overlap at the end of the tubing.

5. True or **False**  Add oil to the open end of your piece of tubing