**Filling the Gap Quiz**

1. True or False Care should be taken not to burn through the wall of the tubing.

2. True or False Complete this process until there is just a small hole in the gap.

3. True or False Weld an overlapping bead across the original pass.

4. True or False You should grind off the weld with an overlap at the end of the tubing.

5. True or False Add oil to the open end of your piece of tubing.